|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | Light Source | LED | | Wave Length | 460nm and 550nm | | Measuring Range | 0-40 mg/dl | | Display | Large Display | | Accuracy | Within 3.5% for values b/w 3.0 - 40 mg/dl Within 5% for values b/w 0.0 - 3.0 mg/dl | | Power Supply | 220V - 50hz | | Dimension | 222mm X 180mm X 100mm | | Printer | 56mm Thermal graphic 384 dots/line | |
|  |