 Main Feature

User friendly icon based operation   
• Calibration cycle: Automatic of programmable: 4 hrs / 8 hrs / standby mode  
• Liquid stable reagents - RFID reagent management inbuilt  
• Universal input voltage 95 to 265 V / 50-60 Hz  
• 8 to 32 GB storage