Feature

• Semi-automatic Single channel coagulometer  
• Printout of the graph and results  
• On-board storage capability up to 20 assays  
• Open system with user friendly software  
• All methods creatable, editable, copy and delete  
• Automated calculation results in seconds, %, INR, g/l, mg/dl, Ratio  
• Calibration/reference curves editable up to 9 measurement points  
• Automatic start-pipette connectable  
• Automated cuvette detection and calculation  
• Data transmission to SD-card or external PC (Optional)